# Configuring a Wireless Client

1. On the sidebar menu, select Configuration .

2. On the Configuration page top bar, select the Network tab.

3. In the upper-right corner of the Network tab, select Edit.

4. Under General, select Enabled.

5. If you want to manually configure your network device, clear the DHCP checkbox and fill out the required information as provided by the local system administrator:

   - IP address

   - Subnet mask

   - Gateway

6. Enter a Network name (SSID).

7. Under Security, select a Mode in the dropdown list:

   - If Disabled is selected, the wireless network will be unsecured.

   - If WPA2 Personal is selected, enter a Security key.

   - If WPA2 Enterprise is selected, enter security parameters and import cert files and keys as applicable.

8. Under Optional, edit the optional settings as applicable:

   - Hostname: type a hostname for the device.

   - Warn on signal strength below (dBm): define below which signal strength value a warning must be activated (default value: -60; value range: -100 - -0).

   - Roaming threshold (dBm): define below which signal strength value the device must search for another access point to attempt roaming (default value: -70; value range: -90 - -45).

   - Connect to hidden WI-Fi network: select the checkbox to enable connection to a hidden Wi-Fi network.

9. In the upper-right corner of the Network tab, select Apply.

   The device will establish a wireless connection to the network.

10. To access the user interface wirelessly, type the device IP address into a web browser.