# Navigating the Measuring Mode

When running an inspection, the STRwrench Controller EHMI automatically enters measuring mode.

The measuring mode opening screen provides the following information on the ongoing inspection:

- Torque limits: lower and upper torque limits values defined for the inspection.

- Joint: name of the joint linked to the inspection.

- Inspection: inspection type.

In the upper right corner of the screen, tap Close to close the opening screen and view information, results and traces related to the ongoing inspection, which are updated in real time and organized in four categories:

- Summary.

- Chart.

- Results.

- Trace.

To navigate the different categories, flick left or right. Alternatively, tap on the name of the category of interest in the top navigation bar.

The bottom bar of the Measuring mode screen displays the following information:

- Inspection name.

- S: number of acquired samples related to the subgroup size configured for the inspection.
  This item is available only for SPC inspections.

- B: number of times the test has been run inside the inspection.

In this Section

- Summary Category
- Chart Category
- Results Category
- Trace Category