# Summary Category

The measuring mode Summary category differs according to the selected inspection type.

Summary category for Cp/Cpk

- Torque limits: the lower and upper torque limits configured for the inspection.

- Test Result: result of the test (OK or NOK).

- Minimum Cp: value of minimum Cp configured for the inspection.

- Cp: value of the Cp index calculated during the test using the measured values.

- Minimum Cpk: value of minimum Cpk configured for the inspection.

- Cpk: value of the Cpk index calculated during the test using the measured values.

Summary category for SPC

- Torque limits: the lower and upper torque limits configured for the inspection.

- X: the average value of the results of the inspection.

- Range: range value according to ISO standard.

- Rules: rules enabled for the inspections and their respective status:

  - Green mark: rule is passed.

  - Red mark: rule is failed.

  - Grey mark: number of values is not enough to assess whether the rule has been passed or not.

Tap on the Rules area of the screen to open the SPC rules check results page, and view the full description of each rule.

Tap Info to open a page displaying the following information on the operation:

- Torque limits: the lower and upper torque limits configured in the inspection.

- Joint: name of the joint linked to the inspection.

- Inspection: name of the inspection running.