# Configuring the ToolsNet Connection

1. On the sidebar menu, select Configuration .

2. On the Configuration page top bar, select External Systems > ToolsNet.

3. In the upper-right corner of the ToolsNet tab, select Edit.

4. Under General, select Enabled.

5. Under PIM, enter the following parameters:

   Parameter | Description
   --- | ---
   Address | Enter ToolsNet server IP address.
   Port | Enter ToolsNet server port. Default value: 9014; value range: 1 - 65535.

6. Under Configuration, enter the following parameters:

   Parameter | Description
   --- | ---
   Station number | Enter the number that ToolsNet must associate to the results collected by STRwrench. Value range: 1 - 9999.
   Station name | Enter the name that identifies STRwrench in ToolsNet tree structure.
   Send traces | Select the checkbox to enable the device to send traces to ToolsNet

7. In the upper-right corner, select Apply.

For further information on how to use ToolsNet 8, refer to ToolsNet 8 User Guide.