# Updating Software Version

During the software update, the connection between the device and the STRwrench QA Inspector Software web user interface must be via USB cable.

The software update cannot be performed if the device is in measuring mode. To proceed with the software update, if you are in measuring mode go back to the STRwrench EHMI home menu. For more information on how to exit the measuring mode, refer to Exiting the Measuring Mode.

1. Connect the STRwrench to the computer via USB cable.

2. Access the STRwrench QA Inspector Software web user interface.

3. On the web user interface sidebar menu, select Integrated Controller Tool .

4. On the Integrated Controller Tool page, select the Software tab.

5. Under Software update, click Choose file.
   Alternatively, drag and drop the zip file with the applicable software version directly into the dedicated field.

6. Browse and select the zip file with the applicable software version.

7. Under Software update, click Update software.

8. In the confirmation dialog, click Yes.

The operation might take several minutes.

The device is automatically restarted for the update to take effect.

Relevant Information

- Accessing the Web User Interface