# Three points residual

- During an inspection, 3 points may appear in the trace result: Residual point, Breakaway point, and Peak point.

- The overall result of the inspection is decided according to the inspection configuration.

- The trace result can be set at the inspection configuration via Web User Interface or via EHMI when the strategy is "Residual Torque/Angle".

- It can also be set as a default configuration at Configuration → Preferences → Inspections default → Torque/Angle.