# Configuring a Wireless Client

1. On the EHMI home menu, tap Configuration > Wireless.

2. In the upper-right corner of the Wireless configuration page, tap Edit .

3. On the General tab, select Enabled.

4. If you want to manually configure your network device, clear the DHCP checkbox and fill out the required information as provided by the local system administrator:

   - IP address

   - Subnet mask

   - Gateway

5. Enter a Network name (SSID).

6. On the Security tab, select a Mode in the drop-down list:

   - If Disabled is selected, the wireless network will be unsecured.

   - If WPA2 Personal is selected, enter a Security key.

   - If WPA2 Enterprise is selected, enter security parameters and import cert files and keys as applicable.

   Use the Web User Interface to edit the TLS and the FAST parameters.

7. On the Optional tab, configure settings as applicable.

   - Hostname: enter a hostname for the device.

   - Warn on signal strength below (dBm): define below which signal strength value a warning must be activated (default value: -60; value range: -100 - -0).

   - Roaming threshold (dBm): define below which signal strength value the device must search for another access point to attempt roaming (default value: -70; value range: -90 - -45).

   - Connect to hidden Wi-Fi network: select the checkbox to enable connection to a hidden Wi-Fi network.

8. On the top bar, tap Apply .

   The device will establish a wireless connection to the network.

9. To access the user interface wirelessly, type the device IP address into a web browser.