# Chart Category

The Chart category displays each value measured during the test positioned in the torque chart.

The torque chart includes the following items:

- Two red lines that represent the upper and lower torque limit values configured for the inspection.

- A green dashed line that represents the target torque value configured for the inspection.

- Grey dots that represent the values measured during each test in the inspection.