# Adding a Joint Inspection

1. On the home menu, tap Joints.

2. On the Joints page, tap the row of the joint you want to add an inspection to.

3. On the Edit Joint page, expand the Inspection category and tap Add on the top bar.

4. In the Test type dialog box, select the inspection type from the following options:

   - Cp/Cpk.

   - SPC.

5. Configure the required inspection parameters in each category.

6. On the top bar of the Add inspection page, tap Apply .

Relevant Information

- Cp/Cpk Inspection Parameters
- SPC Inspection Parameters