# Configuring the Tool

1. On the sidebar menu, select Configuration .

2. On the Configuration page top bar, select the Tool configuration tab.

3. In the upper-right corner of the Tool configuration tab, select Edit.

4. Under General, select or clear the checkboxes to configure the following features:

   Feature | Description
   --- | ---
   Vibration | Selected: Vibration device behaves according to STRwrench ongoing operation. Clear: Vibration device is always off.
   Buzzer | Selected: Audio signaling device behaves according to STRwrench ongoing operation. Clear: Audio signaling device is always off.
   Front LED | Selected: Front LED lights up when the dedicated button is pressed. Clear: Front LED is always off.
   Smart zeroing | Selected: If the STRwrench detects any movement during the zero adjustment, the zeroing procedure will start over again. Clear: If the STRwrench detects any movement during the zero adjustment, the zeroing procedure will not start over again.
   Tag | Selected: Information on the TAG is displayed and can be edited in the Integrated Controller Tool > Tool menu. Clear: Information on the TAG will not be displayed.

5. Under Barcode, select in the drop-down list a barcode mode from the following options:

   Option | Description
   --- | ---
   Disabled | The search of inspections triggered by barcode scan is disabled.
   Only local | The search of inspections triggered by barcode scan is enabled only locally on the STRwrench.
   From QAS | The search of inspections triggered by barcode scan is enabled only on QA Supervisor.

   To be read by the STRwrench scanner, a barcode must contain at least three characters.

6. In the upper right corner of the Tool configuration tab, select Apply.