# 5G Diagnostics

This page describes the real-time view for 5G network signal entities. Information from the following signal entities is displayed:

- Reference Signal Received Power (RSRP)

- Reference Signal Received Quality (RSRQ)

- Receive Signal Strength Indicator (RSSI)

- Signal to Interference plus Noise Ratio (SINR)

- Transmitter Power (TX)

This diagnostic selection is only available when 5G is in the Connected state.

## Start a Diagnostic Session

1. Go to Integrated Controller Tool in the Home menu and select Tool on the left pane.

2. Select 5G Diagnostics in Diagnostics.

3. Select the ellipsis (...) to choose the preferred 5G network signal entity to be monitored.

The graph starts plotting new values every second for the selected 5G network signal entity. Simultaneously, all signal entities will be populated in Radio Quality.

For more information, see also IxB Software User Guide.