# Configuration in Web HMI

After checking the prerequisites, follow these steps to configure the 5G Connect accessory in the Web HMI:

1. In the Home screen, go to the Settings page of the tool.

2. In the Network tab, scroll to the Cellular Network section and press Edit.

3. Switch ON the Cellular Network by using the Enabled toggle.

4. In the APN field, enter the access point name for the 5G network.

5. If necessary, in the SIM PIN field, enter the pin code for unlocking the inserted SIM card and restart the tool.

6. After restarting the tool, go to the Cellular Network section in the Network tab to check the network information and connection status.