# Restoring a Configuration

1. In the upper left corner of the ILM Manager, select the Folder icon.
   Open pop-window opens.

2. In the Open pop-up window, navigate to the location of the XML-file with the configuration.

3. Select the XML-file, then select Open.
   The Configuration window is updated with all ILM devices and configurations from the XML-file.

4. In the Configuration window, select the ILM device to load the configuration to.

5. Right-click the selected ILM device, then select Restore.
   The ILM device's status changes to Pending changes.

   Note that areas are handled separately. In order to restore them, open the tag details by selecting Edit, and select Apply.

6. In the Configuration bar, select the UWB channel that the device is currently configured on.

7. In the Configuration bar, select Upload Configuration.
   The ILM device's status changes to Obtaining, then OK.