# Status LED

The ILM Anchors and ILM Tool Tags are equipped with LED that indicate status.

## ILM Anchor LED Indicator

LED Color | Status
--- | ---
None | No power supply.
Magenta, blinking | The default mode when the ILM Anchor is powered up for the first time. The movement detection is off.
Light Blue | The ILM Anchor is running without configured coordinates.
Green | The ILM Anchor is running with configured coordinates.
Red, blinking | The ILM Anchor has detected a movement.
Dark Blue, blinking | The ILM Anchor firmware is being updated.

## ILM Tool Tag LED Indicators

LED indicator A.
LED Color | Status
--- | ---
None | No power supply.
Green | The ILM Tool Tag is running.

LED indicator B.
LED Color | Status
--- | ---
None | No power supply.
Blue | The ILM Tool Tag is within an enable area.
Green | The ILM Tool Tag is outside an enable area.