# Configuration View

The Configuration view shows all the ILM devices found using Search, and a toolbar with options to configure the ILM system. The tabs below the toolbar can be used to switch between different types of ILM devices shown:

Anchors: shows all the ILM Anchors.
Tags: shows all the ILM Tags and ILM Configurator Sticks.

Any ILM device shown in the Configuration view can be edited by right-clicking on it. This opens a menu:

- Delete: deletes the ILM device from the list.

- Refresh: ignores any pending changes and refreshes the ILM device's configuration.

- Verify: compares the ILM device's hardware configuration with the ILM Manager configuration.

- Restore: changes the ILM device's status to Pending changes. See Restoring a Configuration.

- Replace: opens the Device Replacement window. See Replacing an ILM Anchor and Replacing an ILM Tool Tag.

- Reboot: the ILM device will restart.

- LED Identification: status LED on the ILM device will blink for five seconds.

In this Section

- Configuration Toolbar
- Anchors Tab
- Tags Tab