# Transforming Coordinates

This will transform the coordinates of all ILM Anchors in the ILM system.

1. Save the configuration of the ILM Anchors. See Saving a Configuration.

2. In the Configuration view, on the Configuration toolbar, select Coordinate Transform.
   Coordinate Transformation pop-up window opens.

3. In the Coordinate Transformation window, in the X: and Y: boxes, enter the X and Y value in meters. This value will be added to every coordinate in the system.

4. Select -90° and +90° to rotate the coordinate system. This rotation will be added to every coordinate in the system.

5. Select Confirm.

6. In the Configuration view, on the Configuration toolbar, select Upload Configuration.