# Movement Sensitivity

To protect the ILM system from changes in positions after installation, the ILM Anchor has integrated sensors that detect movement. If an ILM Anchor detects movement, the status LED will start to blink red.

While the status LED is blinking red the ILM Anchor will continue working and running in the configured mode. The status LED notifies the user to verify the ILM Anchor´s position and correct any changes in position.

In this Section

- Configuring Movement Sensitivity
- Resetting Movement Detection