# Configuring an Enable Area

1. In the Configuration view, on the Tags tab, select the ILM Tool Tag, then select Edit.
   Tag Details pop-up window opens.

2. In the Tag Details window, on the Areas tab, choose the area to configure from the Area drop-down list.

3. In the Tightening Program box, enter the Id-number of the tightening program/s.

   This step is only needed when using Confirm and Control mode.

4. Choose what type of area to use:

   - None

   - Rectangle

   - Circle

   - Distances

   Rectangle and Circle uses coordinates and require measured and configured ILM Anchor coordinates, refer to Enable Area Types.

5. Select Teach. The current position and orientation of the ILM Tool Tag will automatically be measured and configured, for Distances with the selected Distance Tolerance in meters as buffer.

   For Rectangle and Circle it is possible to manually adjust the area in Live Area Visualization.

6. Select Use Orientation, and adjust the roll and pitch degrees and the tolerances in the boxes, if needed.

7. In the boxes under the Timeout section, enter the timeout in seconds.

   - Enter Area (s): duration the ILM Tool Tag needs to be inside the area before the tool is enabled.

   - Exit Area (s): duration the ILM Tool Tag needs to be outside the area before the tool is locked.

   - Tag Lost (s): disconnection duration between ILM Anchors and ILM Tool Tag before the tool is locked.

8. Select Apply.

9. Close the Tag Details window.