# Anchors Tab

The Anchors tab in the Configuration view shows the details of all ILM Anchors in the ILM system.

- ANCHOR ID: unique eight character identifier of the ILM Anchor.

- STATUS: current status of the ILM Anchor.

  - Obtaining: ILM Configurator is collecting data from ILM devices.

  - Pending Changes: unsaved changes have been made to the configuration.

  - Configuring: sending configuration changes to the ILM device.

  - OK: data collection complete and configuration updated.

  - Failed: ILM Configurator could not obtain the device.

- GROUPS: groups the ILM Anchor is a part of.

- MOVED: shows if the anchor has been moved/tampered with.

- X: current configured x-coordinate of the ILM Anchor.

- Y: current configured y-coordinate of the ILM Anchor.

- Z: current configured z-coordinate of the ILM Anchor.

- COORDINATOR: shows if the ILM Anchor is a coordinator or not.

- IP ADDRESS: shows the IP address of the ILM Anchor.

- DHCP: shows the DHCP status of the ILM Anchor.

- VERSION: current installed firmware version.

- EDIT DETAILS: the Edit button opens the Details window.

- DELETE: the Delete icon deletes the ILM Anchor from the list.