# Battery Level LED Indicator

The MTRwrench 85 is equipped with a LED indicator that tells the operator if the battery level drops below certain thresholds.

The Battery Level LED behaves as follows:

LED Behavior | Battery charge level | Remark
--- | --- | ---
Off |  | 11% / 15% / 35% - 100% | Battery level suitable for operations. The lower limit of the range depends on the "Low Battery [%]" configuration via MWR-KIT.
Blinking red |  | 11% - 14/28% | Battery level low. The higher limit of the range depends on the "Low Battery [%]" configuration via MWR-KIT (disabled per default: in this case never blinks)
Steady red |  | 0% - 10% | Battery empty.