# Product Data

Operating torque measuring range | 17 [N·m] - 85 [N·m] / 12.5 [lb·ft] - 62.7 [lb·ft]
Drive | 9 x12 mm
Overall length | 212 mm
Weight | 496 g
Operating torque range | from 20% to 100% of the capacity
Mechanical click repeatability | ± 3%
Torque measurement accuracy | ± 3%
Overload capacity | 150 % of nominal capacity
Maximum angular speed | 250 °/s
Angle measurement accuracy | ± 3.6 ° / 360 ° (at 6 ° per second)
Temperature stability of torque measurement | +10 °C to +40 °C (10 °F to 104 °F)
Tightening results memory capacity | 10000 (maximum)
Power supply | Rechargeable NiMH AA battery 1900mAh 1.2V
Radio distance | Up to 20 m This distance can be influenced by various factor: Antenna characteristics: placement of the MTR-KIT antennas can affect range. Environmental conditions: weather, terrain, obstacles, metal parts, can impact signal strength and range. Interference: other electronic devices and signals can cause interference, reducing the effective range