# Cleaning

Keep the MTRwrench 85 clean.

After use, remove any traces of oil and grease from the MTRwrench 85 with a soft cloth and a soft surface cleaner for oil/grease. Do not use aggressive or abrasive cleaner.

Use an anti-static cleaning cloth in order to remove dust from the MTRwrench 85.

Avoid using harsh detergents to clean the MTRwrench 85.

Clean the contact of the MTRwrench 85 by using an electrical contact cleaner solution.