# Torque Control Strategy

The Torque Control Strategy helps the operator achieve the desired target torque, without any angle reading.

The main parameters that define this strategy are the following:

Parameter | Description
--- | ---
Click torque* | Torque target value.
Tightening Program start | Torque value from which the tightening operation starts. Must be ≥ MTRwrench 85 Min torque value.
Minimum Torque | Lower torque limit value.
Maximum Torque | Higher torque limit value.

Parameters with an asterisk are mandatory.

Torque vs. Angle

A | Change screw | E | Minimum Torque
B | Maximum Torque | F | Trigger torque
C | Final Torque | G | Tightening Program Start
D | Click Torque |  |

A result is OK if the Click Torque is within the upper and lower torque limit values defined for the selected tightening program.

For more information on how to configure tightening programs, refer to Power Focus 6000 User Guide or to Power Focus 8 User Guide according to the controller in use.

Relevant Information

- Tightening Operations LED Indicators