# Handling the Wrench

Correct handling:

- Tighten in even strokes.

- Hold the MTRwrench 85 by the middle of the handle when performing a tightening.

- Apply force only in the tightening direction.

- The force applied to the wrench must be one-handed, uniform, parallel and continue until the tool clicks.

- Keep a tightening speed that enables you to immediately stop tightening as soon as the MTRwrench 85 clicks.

Wrong handling:

- Do not apply any force to the wrench after the automatic release (click).

- Do not apply force to the wrench in any direction other than the tightening direction.

- Do not touch the body of the MTRwrench 85 during tightening operations. Positioning the thumb on the tube alters the click value!

- Do not hold the battery housing of the MTRwrench 85 during tightening operations.