# Job Ready LED Indicator

The MTRwrench 85 is equipped with a LED indicator that notifies the operator when a tightening program assigned by Power Focus 6000/Power Focus 8 has been successfully sent to the MTRwrench 85.

The Job Ready LED behaves as follows:

Wrench condition | LED Behavior | Meaning
--- | --- | ---
Wrench inactive | Off |  | Tightening program missing.
Wrench inactive | Steady blue |  | Tightening program received. Wrench ready to operate.
Wrench active | Off |  | Tightening operation ongoing.

Relevant Information

- Configuring Tightening Programs
- Running Tightening Operations