# Configuring the ToolsNet Connection

To connect a controller to ToolsNet and collect tightening results, configure and activate the ToolsNet protocol settings on the controller.

1. On the Home view, select the Settings Tab. Then, on the left, select Server Connections.

2. In the ToolsNet window, set the following parameters:

   Field | Description
   --- | ---
   On/Off | Enables/Disables communication with the ToolsNet server
   Server port | ToolsNet server port
   Server host | ToolsNet server IP address
   Encryption | Use TLS encryption for the ToolsTalk communication

3. Select Apply.

To view the ToolsNet connection status, select the Results icon and go to the Live Results view. Then, select the button. In the appearing dialog box, select the Server connections tab.

For information on how to configure ToolsNet, refer to the ToolsNet 8 User Guide.

Relevant Information

- Viewing Protocol Status