# Abort Sequence and Clear Results - 10127

When signal "Abort sequence and clear results" is set, the ongoing sequence is aborted and signals related to "Clear results" are cleared.

Name in SoftPLC:ABORT_SEQ_AND_CLEAR_RES

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE