# C - Current

Tools
ES STR SL ST SR QST STB IXB

This step restriction is not supported for Power Focus XC.

This restriction checks the actual current where torque passes Torque Trigger. If the actual current exceeds the limits, the tool will be stopped immediately and the tightening program will jump to the next synchronization point or the end of the program. The result will be the first peak or low value, that made the monitor NOK. In case of OK, the result will be the last measured current value. If the torque trigger is never reached during the restriction it will end with status OK.

Parameter | Description
--- | ---
Torque Trigger | Must be >= 0 and < Tool Max Torque.
Low limit | Lowest acceptable current.
High limit | Highest acceptable current.