# Socket Selector External Red Light - 10047

Controls red lights when socket selector is in external mode (how multiple physical devices are mapped to logical sockets are defined by the socket selector resource configuration).

- Byte0 - logical sockets 1-4

- Byte1 - logical sockets 5-8

- Byte2 - logical sockets 9-12

- Byte3 - logical sockets 13-16

- Byte4 - logical sockets 17-20

- Byte5 - logical sockets 21-24

- Byte6 - logical sockets 25-28

- Byte7 - logical sockets 29-32

2 bits per socket, 00=off, 01=flash, 10=solid

Name in SoftPLC: SOCKET_SEL_EXT_RED_LIGHT

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | uint64 | 1 | 64
SocketLedControlTwoDevices | State | uint64 | 1 | 64

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE