# Received Identifier 3 - 194

Signal corresponding to the third configured string in Source batch-string.
Active Identifier String 3 signal is sent in the order the strings/identifiers are received by the system as soon as a string has been received. If running in forced order scan, it is in the configured order, but if running free order scan, 3 might not correspond to the third configured string, but to the third received string.
The strings is the raw received string and not have the "saved position" applied.
Only sent when running Source batch string.

Name in SoftPLC: RECEIVED_IDENTIFIER_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE