# Continue Step - 10128

Continue Step is an input signal that stops the Wait tightening step.
When the tightening has reached a Wait tightening step with the condition Signal configured as Wait Type, a rising edge of the signal Continue Step causes the system (one or more spindles) to release.

For more information, see the sub-signal Channel Command - 10054: Continue Step.

Name in SoftPLC: CONTINUE_STEP

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE