# C - Current

Tools
ES STR SL ST SR QST STB IXB

This monitor measures the actual current at any point after the torque passes Torque Trigger. The result will be the first peak or low value, that made the monitor NOK. In case of OK, the result will be the last measured current value. If the torque trigger is never reached during the monitor it will end with NOK status and no measurement value.

Parameter | Description
--- | ---
Torque Trigger | Must be >= 0 and < Tool Max Torque.
Low limit | Lowest acceptable current.
High limit | Highest acceptable current.