# Max consecutive loosenings reached - 245

Indicates that the maximum consecutive loosenings have been reached and that the tool will be locked until reset by using the signal Reset too many loosenings lock – 10151, or Master unlock – 10005.

Name in SoftPLC: MAX_CONSECUTIVE_LOOSENING_REACHED

Signal type | Value type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: TRUE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: TRUE

- I/O Expander: TRUE