# Stop (state) - 10133

If this signal is set, any ongoing tightening or loosening will be stopped. Will also block any start attempts while set high. Used in combination with 10024 or 10072.

Name in SoftPLC: IN_EXTERNAL_STOP_STATE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE