# Configuration of the Direction Switch

The direction switch on the tool can be configured to trigger certain input signals when switched quickly (with a duration of 500 ms) from clockwise (CW) to counter clockwise (CCW) and back, or vice versa.

## Systems in Remote start

When the system uses remote start and the user wants to trigger a signal assigned to a direction switch in Tool configuration, one needs to assign the respective signal and use the signal 10029 - Select Loosening with a required duration of 500 ms to trigger it. For this to work, an extra configuration step in ToolsTalk is needed. Under Hardware configuration in ToolsTalk, a configuration must be set for the tool by clicking on the tool icon.