# Rh - Rehit

Tools
ES STR SL ST SR QST STB IXB

This restriction checks the torque. If the measured torque exceeds the Detection Torque, the tool is stopped immediately and the program jumps to the next synchronization point (for Power Focus 6000 Synchronized tightening and Power Focus 8 Synchronized tightening), or the end of the program.

It is only possible to add step Rehit restriction to the first step of the multistep tightening program. Once the Rehit restriction has been added to the first step it shall not be possible to move the step to any other position within the tightening program. The Rehit restriction has to be deleted from the first step in order to move it to other position in the tightening program.

Parameter | Description
--- | ---
Detection Torque | If the measured torque exceeds the Detection Torque, the tool is stopped immediately and the program jumps to the next synchronization point (for Power Focus 6000 Synchronized tightening and Power Focus 8 Synchronized tightening), or the end of the program. Must be greater than zero.
Angle Window | The angle window is measured from the start of the step. If no Angle Window is set, the restriction is active during the whole step.