# Pulse Stop - 10030

If this signal is generated any ongoing tightening or loosening will be stopped. Used in combination with 10024 or 10072.

Name in SoftPLC: TIGHTENING_STOP_PULSE

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE