# Triggering Manual Mode

Manual mode can be activated by a switch or an external system. For example (indicated below), a button on an operator panel can be configured to activate manual mode.

1. Go to the Configurations menu and choose Operator panel in the left navigation.

2. If no configuration for an operator panel exists, click the plus icon at the top right of the work space, otherwise continue to the next step.

3. In the configuration you want to alter, click Edit.

4. In the Operator panel configuration window, click on the position [A,B,C,D,E,F,G,I] to configure.

5. In the Position configuration window, click on the Component list. In the list, click One way key switch.

6. Click on the Turn signal list. In the list, choose Manual mode (use the arrow buttons to navigate within the list if necessary).

7. Close the Position configuration window.

If the user needs to be notified that Manual mode has been entered or left, then events 4070 and 4071 have to be configured, respectively.

Relevant Information

- Configuration of Events