# PVTH - Post View Torque High

Tools
ES STR SL ST SR QST STB IXB

This monitor checks that all torque values in the Angle Window Length are below the High limit.

The Angle Window starts at the angle degrees set in Start Angle in reverse direction from the shut-off point. This then spans for the angle degrees set in Angle Window Length in reverse direction. If Start Angle is left blank, the Angle Window starts at the shut-off point. The torque values used in the monitor are based on the mean torque value, calculated over Number of Samples. If the total angle of the step is less than Start Angle plus Angle Window Length the monitor will report NOK.

Parameter | Description
--- | ---
Start Angle | Must be >= 0
Window length | Must be > 0
Number of samples | Minimum value =1 Maximum value = 80
High Limit | Highest acceptable torque.