# Torque Compensation

By using torque compensation, the actual clamping force applied to the joint can be better determined and the scatter in the applied clamping force can be reduced.

The torque compensation point is set by referring back to a specified angle from Rundown complete and calculating a value for the torque used during rundown. This is then compensated for when creating the preload in the screw by adding the torque value calculated in the torque compensation point to the Target torque.

Parameter | Description | Default value
--- | --- | ---
Torque compensation | Enables adjustment if the Target torque for torque used in the rundown step. Off: No compensation is made. On: Manually sets the Torque compensation point. | Off