# ST Selector

The ST selector is a tool accessory. It is installed on the tool and connected to the tool accessory bus. It has a small display, two input buttons and output LEDs.

## Display

The display shows one information at a time and has four different pages that can be configured to display different preset items on every page.

Parameter | Description
--- | ---
Page 1 | Select the message to be displayed from the list: Batch count Current running batch Final angle Final torque Generic IO 1 Generic IO 2 Generic IO 3 Generic IO 4 Generic IO 5 Generic IO 6 Generic IO 7 Generic IO 8 Generic IO 9 Generic IO 10 Remaining batch Selected sequence id Selected tightening program Size of sequence Target/Final torque Target torque Total remaining sequence counter Total sequence counter Total sequence size
Page 2
Page 3
page 4

## Switch time

Parameter | Description
--- | ---
Switch time | Select the time to display one message before the next message is displayed.

## Buttons

The two buttons can be configured to act upon the displayed information and used to step through listed items.

Parameter | Description
--- | ---
Left button | Select one action from the shortcut menu.
Right button | Select one action from the shortcut menu.

## Status LEDs

The status LEDs can be activated or deactivated.

Parameter | Description
--- | ---
Show result LED | Select the desired On or Off radio button.
Show extra LED | Select the desired On or Off radio button.

The result LED are red, green and yellow, and show the same information as the main tool LED.

The two extra LED can show Batch OK and Batch sequence OK. Both these LED are turned off at the next tightening.