# TAW - Torque in Angle Window

Tools
ES STR SL ST SR QST STB IXB

This restriction checks that the measured torque in the Angle Window Length is between the Torque limits. If the measured torque is outside the limits the tool is stopped immediately and the program jumps to the end. The Angle Window Length starts at the Start Angle from the point that the torque first passed the Trigger Torque. If Trigger Torque is not set, then the Start Angle begins at the start of the restriction.

If the end of the Angle Window Length is not reached, the status of the restriction is NOK.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0
Start Angle | Must be >= 0
Window Length | Must be >0
Minimum Limit | Must be >= 0
Maximum Limit | Must be <= Minimum limit