# Post View Torque

Some joints have a torque peak prior to Rundown complete. Post view torque makes it possible to monitor torque values during two specified angular intervals. The interval starts are defined as an angle prior to Rundown complete and torque is then monitored for a specified angular interval.

Post view torque is therefore similar to Rundown torque limits except that the maximum and minimum limits can be positioned independently of each other and can differ in length to better control the outcome of the rundown step.

Parameter | Description | Default value
--- | --- | ---
Post view torque | Post view torque makes it possible to monitor torque values during two specified angular intervals. | Off
Torque min | Torque value for lower Post view torque limit. |
Torque min offset | Angle offset before the Post view torque min interval begins. | 720°
Torque min length | Angle length defining the Post view torque min section. | 90°
Torque max | Torque value for upper Post view torque limit. |
Torque max offset | Angle offset before the Post view torque max interval begins. | 360°
Torque max length | Angle length defining the Post view torque max section. | 90°