# E - Engage

Tools
ES STR SL ST SR QST IXB

This step is not supported for tools configured with Gear Front Attachment (GFA) of type open end.

This step runs the tool in both directions until the socket engages the screw. The step continues until Target torque or Target angle is reached, provided that Continue if not Engaged is set to Yes. If Target Angle is reached in any direction, the direction is reversed. Limit the search iterations by entering Max Engage Attempts. If Target Torque is reached in any direction the step will finish with OK status.

## Microvideo

E- Engage