# Cease

Cease configuration is enabled when an Input/Output Event Boolean signal is selected for a trigger, and is always enabled for an action.

Cease Settings
Setting | Applies to | Description
--- | --- | ---
Time | Trigger Action | The user can set the time (in seconds), with a minimum value greater than 0 and a maximum value less than or equal to 60.
Trigger | The trigger ceases after the specified time.
Action | The action ceases after the specified time.
To Next Tightening | Trigger Action | The trigger or action is reset when the Clear Results - 39 signal is published in the virtual station of the rule.
Trigger | The trigger ceases after the signal is received.
Action | The action ceases after the signal is received.
Defined Signal | Trigger Action | The trigger or action is reset when a user defined signal is received. Reset Virtual Station: Select from the list of available virtual stations. Reset Signal: Select the Boolean IO Signal from the system. Depending on the selected reset signal, the available scenarios are: Event signal: When the event signal is selected as the Reset Signal, then the reset happens when the event occurs. State Signal: When the state signal is selected as the Reset Signal, additional settings can be configured. To configure the state in which the reset should happen, go to Operation and select Equals or Not Equals for the state of the signal, which is True or False.
Trigger | The trigger ceases after the reset signal is received.
Action | The action ceases after the reset signal is received.
Rule State | Action | When the trigger condition is met, the action publishes the user configured output value.