# Toggle CW/CCW For Next Run - 10131

Toggle CW/CCW For Next Run is an input signal which toggles the direction of the SR21/SL tool for the next tightening/loosening.
If the tool is running clockwise, the signal will toggle the direction to counterclockwise.
If the tool is running counterclockwise, the signal will toggle the direction to clockwise.

When the next tightening/loosening is complete, the tool toggles back to the direction it was before the signal was sent.

When the tool is toggled to counterclockwise for the next tightening/loosening, the orange direction LED on the tool blinks.

It is possible to trigger the signal Toggle CW/CCW For Next Run only once.

When the signal toggles the tool direction, any other update of this signal will be neglected.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
Event | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE