# T+A – Tighten to Torque Plus Angle

Tools
ES STR SL ST SR QST STB IXB

This step runs the tool until the target torque is reached. From this point it continues to run an additional target angle.

Parameter | Description
--- | ---
Target torque | The torque target. Must be > 0.
Target angle | The angle target. Must be > 0.
Speed ramp type | Hard, soft, or manual. Default: Hard. If you select Manual, the Speed ramp field opens.
Speed ramp | If Speed ramp type is Manual, this field opens. Default: 500 rpm/s.
Speed | Default: 60 rpm.
Brake (Valid only for Power Focus 6000 Synchronized tightening, Power Focus 8 Synchronized tightening and Flex). | If On the tool will be stopped when the target is reached. If Off the program goes directly to the next step without stopping the tool.

Point and click on image to see more information:

A | Target Torque
B | Target Angle