# Continue Step

If in a Wait tightening step with the condition Signal configured as Wait Type, through the sub-signal Continue Step, it is possible to control tools individually and let the tightening continue.

For more information, see the input signal Continue Step - 10128.

Name in SoftPLC: CHANNEL_COMMAND_CONTINUE_STEP

Value Type | Start bit | Length | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Boolean | 3 | 1 | 1 | 1