# Configuration of the Multiple Transducers

Only available for QST and IxB tools.

Depending on the tool type and the number of transducers, it is possible to set how the torque and angle transducers are used in a tightening. The transducers can be configured to be controlling or monitoring.

Multiple transducers
Parameter | Description
--- | ---
Controlling torque transducer | Set the torque transducer to use for tightening. Available settings: Auto: For QST tools, Torque is used by default. For IxB tools, Torque 2 is used by default. If Torque 2 is not available for the IxB tool type, Torque is used. Torque Torque 2
Controlling angle transducer | Set the angle transducer to use for tightening. Available settings: Auto: For QST tools, Motor angle is used by default. Motor angle Angle Angle 2

Select Details to open a sub-menu with more settings.

Monitor and reporting torque
Parameter | Description
--- | ---
Report monitoring torque values | If set, a Final Torque value will be reported from both the controlling and the monitoring transducer, including evaluation of the status for both (OK/High/Low).
Redundancy error reporting torque | Redundancy error is reported if the Final Torque measured on the controlling transducer differ from the value measured on the monitoring transducer.
Lock the tool on redundancy error | Lock the tool if a redundancy error is detected.

Torque transducer misc settings
Parameter | Description
--- | ---
Require dual torque | If set, the connected tool must have dual torque transducers (that are not disabled) to be able to run a tightening.
Monitoring torque in trace | If set, the values from the monitoring torque transducer are included in the trace.

Dual torque restrictions
Parameter | Description
--- | ---
Enable double torque restriction | If set, the double torque transducer restriction is active.
Maximum torque difference | The limit for the double torque difference restriction.

Monitor and reporting angle
Parameter | Description
--- | ---
Report monitoring angle values | If set, a Final Angle value will be reported from both the controlling and the monitoring transducer, including evaluation of the status for both (OK/High/Low).
Redundancy error reporting angle | Redundancy error is reported if the Final Angle measured on the controlling transducer differ from the value measured on the monitoring transducer.
Lock the tool on redundancy error | Lock the tool if a redundancy error is detected.

Angle transducer misc settings
Parameter | Description
--- | ---
Require dual angle | If set, the connected tool must have dual angle transducers (that are not disabled) to be able to run a tightening.
Monitoring angle in trace | If set, the values from the monitoring angle transducer is included in the trace.

Dual angle restrictions
Parameter | Description
--- | ---
Enable double angle restriction | If set, the double angle transducer restriction is active.
Maximum angle difference | The limit for the double angle difference restriction.