# Channel Command - 10054

Channel Command is an input signal that inhibits individual tools and prevents that those tools are included in the next tightening. It is also possible to replace the tightening program or bolt number configured in the sync mode configuration. Up to 64 channels are supported.

Name in SoftPLC: CHANNEL_COMMAND

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | uint32 array | 1 | 64

The signal Channel Command -10054 contains sub-signals (for more information, see "Input Signals: Sub-signals").

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: TRUE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE